Foot Path – Broadway 

The main footpath either side of the broadway development is approximately 40mm above road level rising to 120mm above road height within the last few curb edgings either side of the broadway development (see photo “view to 57.2” & “view to 63”) 
The owner of number 63 Broadway has said if a heavy rain fall the rain water already seeps into his property and is concerned that a raise in curb edging height could flow excess water to the front of his property. The front door to his property opens at footpath level without a step up to the door threshold and water pools outside his front door (see photo “outside 63 Broadway -2”). 
The proposed foot path height would be to continue the approximately 40mm above road level along the entire frontage. This height would work well with the paving curb bordering the properties build on the development (see photo “footpath level to property”) 
[bookmark: _GoBack]The foot path is to be placed over the existing road / entrance into the former petrol station therefor the sub base is highway spec and does not need replacing, A channel will be cut into the tarmac surface and a curb edging concreted in place, the foot path level will be built up to the top of the curb using a primer, base tarmac and topping tarmac. 

