Appendix VI – Results Summary

Soil Test results from WAC test summarised and compared to Soil Guideline Values (SGV’s)

	Determinand
	Report No 47973-21
	Report No 47974-21
	SGV’s

	
	Sample No ENV 59806
	Sample No ENV 59807
	

	
	Sample 1
	Sample 2
	

	pH
	8.3
	8.7
	

	Copper
	0.07
	0.10
	200

	Zinc
	<0.5
	<0.5
	300

	Lead
	<0.05
	<0.05
	300

	Arsenic
	<0.05
	<0.05
	37

	Cadmium
	<0.01
	<0.01
	22

	Nickel
	<0.05
	<0.05
	130

	Chromium
	<0.05
	<0.05
	130

	Mercury
	<0.005
	<0.005
	10

	Selenium
	<0.01
	<0.01
	350

	Molybdenum
	<0.05
	<0.05
	4

	Fluoride
	4
	2
	500

	EPH (C10-C40)
	397
	736*
	500

	Total Organic Carbon
	10.1
	6.6
	

	Organic Matter (LOI)
	10.8
	6
	




Notes on results;
· SGV guideline level comparisons are taken from the CLEA model & Environmental Permitting Regulations and other linked legislation.
· All results are expressed in mg/kg unless otherwise stated and represent the maximum permissible in soil.
· The pH level in both samples are high at 8.3 to 8.7.
· At low pH levels, PTE’s become more available to plant uptake therefore to a large extent, pH will govern permitted levels.
· EPH includes category 1 & Category 2 products.
· EPH levels exceeded on sample 2. Mitigation measures include importation of clean ‘fill’ material to cover existing by 300mm+
· Assumed land use is ‘Residential use with plant uptake.’

