Moulton seas End War memorial 
Work instruction for Cleaning 

1. Ist clean with a little bleach and dilute with water starting at the foot of memorial working upwards useing scrubbing brushes 
Rinse down after first clean with water 
2 . Starting from foot of memorial 
2nd clean useing granite cleaner diluted in a bucket brushing cleaner on whole memorial ,more scrubbing to get best results . Then rinse whole memorial down once again 
Step ladders will be used to get above height of memorial one man holding steps , one man cleaning and rinsing 
Cleaner to be used will be 
Ammonium hydrogen dyfloride 
All Ppe to be warn when administering granite cleaner and rinsing off , rubber gloves . Masks and safety glasses, 
3. When memorial all clean and dry black enamel paint will be used to repaint all lettering names and designs 

