Moulton Seas End War Memorial
Method of cleaning.

The monument is in good condition with no cracks or crevices to allow water to penetrate. Small dirt deposits are noted but very little biological growth.
Lightly brushing away the dirt and mineral deposits, before applying plain  distilled water without any chemicals.
Cleaning will be done using a small bristle brush in round movements working from the top down. Care will be taken around any painted wording and carved detail. Regular checks will be done during this process so as to not allow any streaking.
Repainting of some of the wording in black paint same as used when the monument was constructed.

