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	Your name/company:     BK&MORE LTD

	
	Name and address of client: AS&S Property investments Ltd, 21 Brownlow rd Peterborough PE1 3PN

	
	Contact details of architect or principal designer: Ken Mwaniki, ARB, RIBA, Phi Architectural Design (PAD) Ltd
07811199947

	
	What is the job?   Internal Building work

	
	Key dates: Start   27.12.2022                           Finish     20.08.2023                           

	
	Where are your toilet, washing and rest facilities?  Inside building, ground and 1 floor

	WORKING TOGETHER
	Who else is on site - and their contact details?
	Company subcontractors and supervisors
	07561400732
07572774872

	
	Who will be the principal contractor?
BK&MORE LTD

	
	How will you keep everyone on site updated during the job?
pre-construction meeting in morning, information board, Signs

	ORGANISE
	What are the main dangers on site, e.g.:
	Hazard is present
	What controls do you have?

	
	Exposure to building dusts
■ Prevent dust by using wet cutting and vacuum extraction on tools: use a vacuum cleaner rather than sweeping; use a suitable, well-fitting mask
	

Yes
	Water is often used to dampen down dust clouds. Enclose work tops to help stop any dust escaping. Limit the number of people near the workspace and rotate those doing the task regularly. On-tool extraction or general mechanical ventilation

	
	Exposure to asbestos
■    If you suspect that asbestos might be present, don't start work until a demolition/refurbishment survey has been carried out
■    Make sure everyone on the site is aware of the results
	 

Yes
	Very low risk material. Will be
removed by asbestos surveying ltd
Ktween@asbestossurveyingltd.co.uk

	
	Electricity
■    Turn electricity supply and other services off before drilling into walls

	

Yes 
	 Ensure that workers know how to use the electrical equipment safely
 Check that socket outlets are not overloaded by using unfused adaptors as this can cause fires
Ensure there are no trailing cables that can cause people to trip or fall
Switch off and unplug appliances before cleaning or adjusting them
Ensure everyone looks for electrical wires, cables or equipment near where they are going to work and check for signs warning of dangers from electricity, or any other hazard. Checks will be made around the job, and remember that electrical cables may be within walls, floors and ceilings (especially when drilling into these locations) etc

	
	Risks to members of the public, the client and others
■ Keep the site secure to prevent unauthorised access.
	 
Yes
	Car park (Drapers Place ) is secure with fencing panels and safety
signs. Personal vehicles during day
time keep in property secure car
park.
All deliveries (Materials) will be
delivered by Van once in week,
except Fridays.
No work, or deliveries on market
place side.

	
	Vibration
	Yes
	Use high-quality, low-vibration tools.
Use the right tool for the job.
Follow manufacturer instructions for use and maintenance.
Inspect and maintain power tools regularly for wear and damage that could increase vibration exposure.

	This guidance is issued by the Health and Safety Executive. Following the guidance is not compulsory, unless specifically staled, and you are free to take other action. But if you do follow the guidance you will normally be doing enough to comply with the law. Health and safety inspectors seek to secure compliance with the law and may refer to this guidance.
HSE: https://www.hse.gov.uk/
CLC : https://www.constructionleadershipcouncil.co.uk/

	© Crown copyright If you wish to reuse this information visit www.hse gov.uk/copyright.htm for details.

	Published by the Health and Safety Executive
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