1. Drive View – Existing double skin Wall
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2. Drive View - Proposed Step Increase of 150mm at A.  Max Height <2m
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3. Side View Existing
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4. Side View – Proposed Stepped increase at :
A= 150mm. B = 300mm C= 450mm.  Max Height 2m
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150mm increase 
C = 450mm increase
B = 5m Length
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5. Front View  Existing
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6. Front – Proposed increase c450mm Max Height <2m
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