Roman Lodge, Mill Lane, Tydd St Mary, Lincolnshire. PE13 5SB
Following a recent break-in (crime Ref: 19000227422) on the evening of Friday 3rd May 19 and, following a lack of police response we now recognise the need to improve the preventative and detective security controls that protect our home . The existing intruder alarm while fitted, does not have an external alarm box so has in effect never been fully operational.  We assume that this is because planning permission has not been previously requested.  

Proposal - 
Alarm System:
We propose to upgrade all existing internal security sensors (Motion and Door ) with modern wireless units.  This requires no wiring and will not impact in any way on the fabric / look of the building.  The original alarm internal control box was located by the main electric fuse box in the basement.  This has been replaced with a modern equivalent in order that we can link both garden sheds to the alarm system and protect expensive garden equipment.  Cabling has been required but it was undertaken using existing drill holes in the basement and by trenching power and other cables via a conduit through the garden.  This work has not impacted on the fabric / look of the building, has been undertaken to appropriate electrical standards and will be certified by a fully qualified electrician upon full completion.  
In order to ensure an effective alarm system we request permission to place an external "bell box" to the from of the house.  An indicative position is shown on attachment "Alarm Box B".  The external cables follow and secure to the existing TV areal cable and again, other than the three small drill holes requited to fasten the box to the wall, there will not be any significant impact to the building.  We prefer to use black cables and alarm box to maintain consistency with the existing guttering etc.

CCTV:
 Due to our location and ease of access to our grounds and buildings via open fields as well as by a small private lane, we would also like to request permission to add a discreet (but still visible) CCTV system around the house.  With respect to the camera coverage required for the (listed) house, we propose 4 discreet (but still visible) cameras.  Approximate locations are shown on 4 attachements (House Floor Plan, Camera 1&2, Camera 3, and Camera 4).  The majority of cabling will run along guttering / drain pipes.  Cable clips will be required in some instances but their use causes no more damage than the existing fixings used to secure trellis at various locations around the house.  Cables will be feed to the basement (again using an existing cable route) for attachment to a new CCTV recorder / control box to be located by and connected to the electric fuse box in the Basement.
Cameras proposed are HIKVISION  DS-2CD2349 (with mounts - see Attachments Camera White , and Camera Black - We propose to use Black if acceptable to you. 
