Caravan act:

The timber building quoted for can adhere to the Caravan Act with regards to mobility. 
The building can be split and transported in two 'units' and bolted back together on site. The felting, shingles roof covering can link together as the two units meet and a protective strip added down the seam if necessary. No glue is used here, therefore any tacking nails can be removed & the units unbolted again when the structure is due to be moved. Our proposed site is also designed in such a way that access to move the building at a later date will be straight forward.
The proposed building floor area is also now just under 30m2
The roof height has also been reduced down to approx. 3m
It is fully insulated (walls, floor and roof) and includes 24mm sealed toughened double glazing to insulate.

