
Fast-3550MM-S
Fastensol 3550mm Silver Rail
The mounting rails are the core of the system. For each row of panels, a pair of rails is mounted horizontally on the roof and supported by rook hooks at no more than 1.2m intervals. The distance between the rails should be around three-quarters of the panel height. The panels are then laid on the rails and clamped in place with the end and mid clamps.
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Overview
For long rows, simply join lengths of rail using the rail splice kits. Rails can be cut to length with a hacksaw or grinder.
System features and specifications:
· Dimensions: 3550 x 50 x 29 mm
· Suitable for pitched and flat roofs
· Cladding type: tiled, slate and sheet metal (other roof mounts also available)
· Maximum slope: 60 degrees
· Wind load: up to 60m/s
· Snow load: 2.0kn/m2
· Maximum building height: 20m
· Material: aluminium
· Color: silver
· MCS 012 certification
· Warranty: 12 years durability on material, 5 years on finish
· Manufacturer: Xiamen Fasten Solar Technology Co., Ltd
· 561 rails per pallet cage
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