Conceptual Site Model of Contamination			Appendix IV				

Site; Railway Cottage, Counter Drain Drove, Tongue End, Spalding.


	Source
	Pathway
	Receptor
	Estimated Risk

	Soils impacted by petroleum hydrocarbons, heavy metals.  Asbestos fibres and fragments – confirmed none present.
	Direct or dermal contact with soil
	On site workers during demolition/ remedial works, excavation and/or development. Site visitors during development.


Ecology





Buildings and infrastructure.




Local offsite tenants and neighbours and future occupiers




Future site occupiers.
	Moderate – potential for direct contact with contaminated soils





Low – Existing vegetation within site  and site perimeter appears to be healthy.

Low – soil conditions do not appear aggressive to building materials.

Low – Hard landscaped area or where soils are capped.




Low






Conceptual Site Model of Contamination – continued


	Source
	Pathway
	Receptor
	Estimated Risk

	Groundwater impacted by heavy metals and Petro Hydrocarbons, PTE’s
	Contact with water, vertical and horizontal migration through to surface waters, adjacent ditch & Counter drain.
	On site workers during demolition/ remedial works, excavation and/or development.



Ecological systems

Buildings and Infrastructure.


Local off-site tenants.



Future site occupiers

	Low – minimal, works undertaken above water table. 





Low

Low – foundations are to be above water table.

Low – minimal groundwater impact and depth to groundwater.

Low – minimal groundwater impact.






