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MegaStor Galvanised Steel Water Storage Tank
Description:

‘The steel support structure of an MegaStor tank is engineered for strength and durabilty,
with a built-in 40% safety margin to ensure long-term reliabilty.

Product Overview:

Variants: Available in short and long panel options to suit different space requirements
‘Capacites: From 2m® to 2000, ideal for residential, commercial, and industrial use.
Easy Installation: Designed for quick setup with step-by-step guides.

Portable: Compact and easy to transport, perfect for mabile or remote applications.
‘Scalable: Link tanks in series or paraliel to increase capacity as needed.

Flexible: Fully demountable for temporary or relocatable storage.

Versatile Installation: Can be installed above ground, half-buried, or fully buried
Customisable: Powder coating available in various colours to suit your site or branding.
Multi-Use: Suitable for storing other liquids, not just water.

"MegaStor Water Tank Base Requirement nstallation Details:

Tank Tank Minium | Concrete | Sand
Diameter | Diameter | Base Required | Required

Fainstor (Meters) | (Feet) Diameter | (m3) (m3)
. Meters)

3.81m Height

Workingin partershipwitn | 1189 3 1249 1225 555
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Steel MegaStor with Powder Coated

Description:

Powder-coated galvanised steel tanks offer several key benefits. The durable
coating adds an extra layer of protection against corrosion, weathering, and
‘general wear, increasing the life expectancy of a standard tank by up to 50%.
This powder coating can be applied in any colour, giving you the flexibility to
match the tank and roof to your site’s surroundings or company branding,
Both the tank body and the galvanised roof can be coated, ensuring a uniform
‘and visually appealing finish across the entire system.
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