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1
DEVELOPMENT DESCRIPTION AND LOCATION.

1a
Type of development and Location
The proposal is for the construction of 2 No Stables with Tack Room The site is adjacent to Bridge farm Fen Road Holbeach Lincs PE12 8QF
1b
Vulnerability Classification

The development falls within Zone 3 of the Environment Agency Flood Map.
1c
Local Development Documents


The proposal is consistent with the relevant aspects of the Local Development Plan.

1d
Sequential Test/Exception Test


The site is 0.30 hectares and is for a Non Residential Development.

In terms of the sequential test there is no other similar land in the vicinity in the ownership of the applicant for the purposes of the test there is no other suitable land, or any alternative land that is at less risk in the immediate locality.

2
DEFINITION OF THE FLOOD HAZARD.

2a
Sources of flooding that could affect the site.

The primary possible source of flooding of the site would be either from rivers or the sea, if there were no flood defences. This area could be flooded:

· From a river by a flood that has a 0.5 % (1 in 200) or greater chance of happening each year.


Extreme rainfall could be another possible cause of flooding. 
2b
Identified flooding sources – how they might affect the site.


Fluvial flow and overtopping of the embankments would not inundate the site rapidly as the site is located further away from the source than much of the more prone areas closer to the sea or river. Any flooding scenario would be likely to be signalled well in advance with flood warnings, weather reports and local observations as to water levels within the river.

Extreme rainfall on the site should not have a major effect, as the site stands alone, has well drained surfaces. 

2c
Existing surface water arrangements.


The adjacent and existing properties are served by soakaways.

3
PROBABILITY

3a
Flood Zone

The site is within Flood Zone 3
3b
Existing Surface water rates and volumes of run off generated by the site.

The site will not generate any significant additional surface water runoff.
4
CLIMATE CHANGE

4a
How is flood risk at site likely to be affected by climate change


The site may be at risk if sea levels and river flows increase with climate change. 

The site may be at increased risk if rainfall increases with climate change.

In mitigation the proposed dwellings can be built in accordance with e the latest Environment Agency recommendations thus reducing any risk to a minimal level.
5
DETAILED DEVELOPMENT PROPOSALS.

5a
Details of the proposed development


Please see drawings Numbered 1716-01
Application for 2 No Stables with Tack Room 
6
FLOOD RISK MANAGEMENT MEASURES
6a
How will the site be protected from flooding, including the potential impacts of climate change over the developments lifetime.


The site sits some distance away from any rivers the nearest being the Nene on which the banks have been strengthened and raised and there are large areas of flood plain adjacent to the river.


The site sits some distance away from the sea and the existing defensive banks are in good condition. They were not breached in the 2013 tidal surge.


The Site is not within a Functional Floodplain. It is located in the Passive Floodplain protected by existing tidal defences.

Although the site is located in Zone 2 the actual risk of Flooding from the river Nene system is very low (less than 0.5%)

There is no Habitable accommodation provided by this application.
