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	33 Bridge Road, Long Sutton, Spalding, PE12 9EF

SITE PLAN – INCLUDING PROPOSED ALTERATIONS ENLARGED
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Map area bounded by: 544053,322404 544143,322494. Produced on 11 March 2021 from the OS National Geographic Database. THReproduction in whole or part is prohibited without the prior permission of Ordnance Survey. © Crown copyright 2021. Supplied by UKPlanningMaps.com a licensed OS partner (100054135). Unique plan reference: b90cuk/591213/801666-2


NEW DRIVEWAY ACCESS / DROPPED KERB








1 INSPECTION CHAMBER 1200MM X 750MM  WITH CATCH PIT 200MM BELOW PIPEWORK LEVEL, CONSTRUCTED FROM 2 COURSES OF ENGINEERING BRICKS UP TO TWINWALL PIPE, THEN RISER CONSTRUCTED FROM REINFORCED CONCRETE RINGS. THIS WILL CONNECT 2 GULLEY OUTLETS TO 300MM TWIN WALL PIPE AND COMPLETED WITH REINFORCED TOP SLAB AND INSPECTION LID, ALL PLACED ON REFORCED CONCRETE BASE.


 TREE MARKED T1 ON EXISTING SITE PLAN TO BE REMOVED

















RED HATCHED AREA SHOWING PROPOSED CULVERT EXTENSION WITH PIPE AND RELEVANT CHAMBERS, AREA “A” TO BE GRAVELLED, BLUE LINES SHOWING PROPOSED FENCE LINE ( HEIGHT 2M )


WEST FENCE 2 METRES FROM WATERCOURSE EDGE AFTER REMOVING TREES


SOUTH FENCE RUN ALONG EXISTING DYKE
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PIPEWORK TO TERMINATE 300MM PROUD OF BANK LEVEL,


BANK TO BE BATTERED TO MATCH EXISTING SLOPE AND FINISH HEIGHT











