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	33 Bridge Road, Long Sutton, Spalding, PE12 9EF

SITE PLAN – INCLUDING PROPOSED ALTERATIONS ENLARGED
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2 INSPECTION CHAMBERS 1200MM X 750MM  WITH CATCH PITS 200MM BELOW PIPEWORK LEVEL, CONSTRUCTED FROM 2 COURSES OF ENGINEERING BRICKS UP TO TWINWALL PIPE, THEN RISER CONSTRUCTED FROM REINFORCED CONCRETE RINGS. THIS WILL CONNECT 2 KERBSIDE DRAINS TO 300MM TWIN WALL PIPE AND COMPLETED WITH REINFORCED TOP SLAB AND INSPECTION LID, ALL PLACED ON REINFORCED CONCRETE BASE





NEW DRIVEWAY WITH DROPPED KERB








RED HATCHED AREA SHOWING PROPOSED CULVERT EXTENSION WITH PIPE AND RELEVANT CHAMBERS, AREA “A” TO BE GRAVELLED, BLUE LINES SHOWING PROPOSED FENCE LINE ( HEIGHT 2M )


WEST FENCE 2 METRES FROM WATERCOURSE EDGE AFTER REMOVING TREES


SOUTH FENCE RUN ALONG PATH
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PIPEWORK TO TERMINATE 300MM PROUD OF BANK LEVEL,


BANK TO BE BATTERED TO MATCH EXISTING SLOPE AND FINISH HEIGHT











