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Method Statement for the demolition of buildings at Spalding Road, Pinchbeck

· All services to be disconnected prior to demolition commencing.

· Site to be fenced using 2m high block and mesh type fencing prior to work commencing.

· Building to be soft striped by hand, removing all loose furniture, fixtures and fittings etc.

· All arising materials to be loaded onto trucks for removal off of site.

· [bookmark: _GoBack]Asbestos/cement roof sheets to be carefully removed by hand, by men working from M.E.W.P’s and all arising materials to be placed into skips for disposal off of site.

· 360 JCB excavator to demolish remaining structures, including floor slab and foundations where necessary

· All arising materials to be loaded onto lorries for recycling off of site.

· Site to be left in a clean, tidy and safe condition at the end of each shift and upon completion of works.

· All relevant PPE and RPE to be worn at all times where necessary.

· All work to be carried out following all current HSE guidelines.

· All plant on site to hold up to date test certificates and to only be operated by competent operators holding up to date CPCS card or equivalent. 
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