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Appendix F. Road safety audit response report template for stages 1, 2 and 3 only
[bookmark: F1_Project_details][bookmark: _bookmark70]F1	Project details
Provide:
Table F.1 Project details

	Report title:
	RSA1 Designer’s Response

	Date:
	17.04.26

	Document reference and revision:
	Rev 1

	Prepared by:
	AMA Ltd 

	On behalf of:
	Lincolnshire County Council


Table F.2 Authorisation sheetDownloaded from https://www.standardsforhighways.co.uk on 13-Feb-2024, GG 119, published: Jan-2020

	Project:
	Proposed food store and drive-thru development, Holbeach Road, Spalding

	Report title:
	RSA1 Designers Response

	Prepared by:
	

	Name:
	Robert Wickenden

	Position:
	Senior Transport Planner

	Signed:
	

	Organisation:
	AMA Ltd

	Date:
	17.04.26

	Approved by:
	

	Name:
	Alex McGarrell

	Position:
	Associate Director

	Signed:
	

	Organisation:
	AMA Ltd

	Date:
	17.04.26


[bookmark: F2_Introduction][bookmark: _bookmark71]F2	Introduction
As part of the Transport Assessment (TA) that accompanied a planning application (Ref: 25/0704/FUL) for a food store and drive-thru. Andrew Moseley Associates (AMA) designed the left in / left out / right in only priority-controlled T-junction on Holbeach Road in Spalding.
The proposals have now been subject to a Stage 1 Road Safety Audit (RSA1) carried out by Jon Birkett and Naomi Cook on Thursday 14th April 2026.
Rob Wickenden (Senior Transport Planner) and Alex McGarrell (Associate Director) of AMA Ltd prepared the Stage 1 Road Safety Audit Designer’s Response.

[bookmark: F3_Key_personnel][bookmark: _bookmark72]F3	Key personnel
Provide:
Table F.3 Key personnel

	Overseeing Organisation:
	Lincolnshire County Council

	RSA team:
	Jon Birkett / Naomi Cook

	Design organisation:
	AMA Ltd





F4	Road safety audit decision log
Insert RSA decision log. This can be a spreadsheet appended to the RSA response report.
Table F.4 Road safety audit decision log

	RSA
problem
	RSA
recommendation
	Design
organisation response
	Overseeing Organisation response
	Agreed RSA action

	Problem 1.1: General to the scheme

Increase in collisions resulting from ineffective surface water drainage. 

No details of any proposed highway drainage works have been provided as part of the RSA information. The proposals include the alterations and widening of the A151 Holbeach Road and introduce additional impermeable surface. If surface water cannot drain effectively there is a risk of surfacing water ponding and encroaching into the wheel paths of vehicles on the internal highway network. This can result in a loss of friction and subsequent collisions resulting from aquaplaning or loss of control.

	Provide effective highway drainage to ensure A151 Holbeach Road can operate safely during wet weather conditions.
	Highway drainage will be dealt with the S278 detailed design stage.
	
	

	Problem 1.2: A16 and A151 Holbeach Road

Increase in collisions due to insufficient lighting levels.

The proposed junction will a number of the street lighting columns which if not relocated to an appropriate position will result in the accesses and vehicles using it being in shadow during the hours of darkness or low light conditions and could result in an increase in collisions associated with vehicle and pedestrian
movements during the hours of darkness. There is also a risk of cyclists and pedestrians being unseen by drivers, as they cross the access junctions or cycle along Holbeach Road and Low Road, resulting in an increase in collisions.
	Review the need for street lighting and, if appropriate, include detailed design.
	Street lighting will be dealt with at the S278 detailed design stage.
	
	

	Problem 1.3: Site access junction

A lack of signing and lining will increase the risk of cross path collisions.

A new access junction will be created which allows all movements except right turn manoeuvres out of the new development onto Holbeach Road. The drawing provided does not show any signing or road markings that would reinforce this restricted turning movement which could in turn lead to vehicles making a right turn increasing the risk of cross path collisions and head on collisions.

	At detailed design, include appropriate signing and road markings to reinforce the restricted movements for vehicles exiting the development.
	Appropriate signage and road markings will be dealt with at the S278 detailed design stage.
	
	

	Problem 1.4: Site access junction

A lack of suitable crossing points will increase the risk of collisions between pedestrians and vehicles on Holbeach Road.

A new uncontrolled crossing is proposed over the development access and a short section of footway around the eastern radius of the access junction. This footway terminates leaving pedestrians with two options, the first to walk in the verge increasing the risk of trips and falls and secondly to cross the A151 Holbeach Road. The drawings do not show any crossing facilities at the A151 and due to the busy nature of Holbeach Road pedestrians will likely have to wait within the central hatched area increasing the risk of being struck by a passing vehicle.

	At detailed design carefully consider the need to provide a suitable crossing point of the A151 Holbeach Road to the east of the access junction. Alternatively, depending on demand and desire lines, omit the footway on the eastern radius as well as the proposed crossing point across the junction.
	The issue is noted. Upon a further review, pedestrians can cross the A151 Holbeach Road at the splitter island on the eastern approach to Springfield Roundabout.
	
	

	Problem 1.5: Site access junction A151 Holbeach Road.

Inappropriate carriageway widths and turning radii can result in increased vehicle collisions as well as pedestrian-vehicle collisions.

Details of the swept paths of vehicles are not provided on the drawings. Inappropriate carriageway widths and junction radii can result in vehicles failing to safely negotiate the new junction arrangements and will increase the risk of vehicle collisions and pedestrian-vehicle collisions.

	Ensure that the proposed access junction is of sufficient size to accommodate the needs of the development.
	The site access has been assessed with swept path analysis using a 16.5m max legal articulated HGV. The site access on Holbeach Road has been amended to ensure that the manoeuvre is very tight to deter delivery vehicles from entering the site via this point. Furthermore, servicing will only take place via the left in only access from the A16 Low Road.
	
	

	Problem 1.6: Site access junction A16 Low Road.

A lack of separation between NMU’s and vehicles will increase the risk of injury to NMU’s.

It is proposed to construct a new entry only junction off the A16 to the south of the Springfields Roundabout. Currently there is a 0.5m wide separation between NMU’s and the existing shared use route. The proposed drawing does not show any separation. A lack of separation between NMU’s and vehicles will increase the risk of injury to NMU’s.

	Retain the existing separation between vehicles and the MNU route along the new access junction.
	A section of verge in line with the existing will be provided between the carriageway and footway / cycleway as part of the S278 detailed design.
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F5	Design organisation and Overseeing Organisation statements
Include the following statements to be signed by the design organisation and the Overseeing Organisation.
Table F.5 Design organisation statementDownloaded from https://www.standardsforhighways.co.uk on 13-Feb-2024, GG 119, published: Jan-2020


	On behalf of the design organisation I certify that:
1) the RSA actions identified in response to the road safety audit problems in this road safety audit have been discussed and agreed with the Overseeing Organisation.

	Name:
	Alex McGarrell

	Signed
	

	Position:
	Associate Director

	Organisation:
	Andrew Moseley Associates Ltd

	Date:
	17.04.2026




Table F.6 Overseeing Organisation statement

	On behalf of the Overseeing Organisation I certify that:
1) the RSA actions identified in response to the road safety audit problems in this road safety audit have been discussed and agreed with the design organisation; and
2) the agreed RSA actions will be progressed.

	Name:
	

	Signed:
	

	Position:
	

	Organisation:
	

	Date:
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