Access, Design & Heritage Statement
Site Address: LLOYDS BANK, HALL PLACE, SPALDING, LINCOLNSHIRE PE11 1SF
Amount:
The scheme includes the provision of keyline lighting beneath a stone band running full length around the ground floor shopfront. The coverage of area with this feature is restricted to the dimension of the stone band.
Scale:

The existing and proposed signage sizes are detailed below.

	Signage
	Existing (mm)
	Proposed (mm)

	Keyline Lighting
	N/A
	4898w x 40h
8660w x 40h

10,815w x 40h

3000w x 40h approx. (curve)


Landscape:  

There is no immediate plan to landscape this area as a result of this development.

Appearance:   

The keyline lighting will also be lit by LED’s, the colour of which when illuminated will be green. The lighting strip will be contained within an aluminium channel painted to blend in with colour of stonework.
Lighting Assessment:

The proposed lighting will be internally illuminated using LED’s and will be wired to the power supply inside the property. The method of illumination will be non-intrusive and in context to the Built Heritage of the surroundings.  
Access: 

Access to the property will be unaffected by this proposal to replace signage.

List Description:
 Mid-late C19. 2 storeys in red brick with ashlar dressings and slate roof, rounded to corner, with red ridge tile and ornamental chimney stacks. Carved ashlar cornice of modified anthemion pattern. Windows are 3-2 and 1 to corner and 4 to Red Lion Street elevation. All with rectangular drip moulds, with flat arches and mask terminals to ground floor and segmental arches and foliated terminals to 1st floor. Doorway to west on ground floor has similar drip mould. 1st floor windows have ashlar aprons and string between storeys. Ground floor has band at cills and ashlar plinth. Main doorway to corner has elaborately carved pointed ashlar gable, terminating in a carved poppy-head finial. Carved spandrels and round-arched doorway.
Proposal:

Installation of keyline lighting fitted directly below stone feature running full length of shopfront. The existing letters, projecting and roundel signage will remain in situ and do not feature in any new advertisement/listed consent application.
Impact upon Building and Conservation Area:

There will be minimal impact on the building and locality. The new signage is in keeping with the style of the listed building ensuring appearance is consistent and attractive. 
Scheduled Installation:

Installation date set for Spring 2016 (by 31st March) and depending on advertisement / listed consent. This will involve a small installation crew who will visit the site and installing new lighting proposed within a timeframe of 1-2 working days. Installation crews will also carry out risk assessments and implement appropriate safety measures to ensure the safety of themselves and others while on site.

